Back EMF problem - attach a Schottky diode

In-rush current problem - DON’T give 100%duty cycle PWM instantly to the motor, ALWAYS start with 0% and slowly increment to what every duty cycle you want