* Using IRQ pin with every interrupt, we check wether ouput b is on when output a is on,

If yes, we increment a “counter” variable, if no then we decrement

* Must enable interrupts, GIE, PEIE and INTE
* Must choose INTEDG bit which determines when does the IRQ pin send an interrupt